
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "104031-0811" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 13.462 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "104031-0811" (id 1) (at -12.7 -15.24 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "MOLEX_104031-0811" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "B2" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.57mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Molex" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "104031-0811_0_0"
      (rectangle (start -12.7 -12.7) (end 12.7 12.7)
        (stroke (width 0.1524)) (fill (type background))
      )
      (pin bidirectional line (at 17.78 0.0 180.0) (length 5.08)
        (name "DAT2"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "CD/DAT3"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 0.0 0) (length 5.08)
        (name "CMD"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 10.16 180.0) (length 5.08)
        (name "VDD"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at -17.78 5.08 0) (length 5.08)
        (name "CLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -7.62 180.0) (length 5.08)
        (name "VSS"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 5.08 180.0) (length 5.08)
        (name "DAT0"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 2.54 180.0) (length 5.08)
        (name "DAT1"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "G1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "G2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "G3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "G4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -5.08 0) (length 5.08)
        (name "SW-1"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -17.78 -7.62 0) (length 5.08)
        (name "SW-2"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)